Cino USB Virtual COM Driver for Windows Systems


*Software Revision
Cino_USB_VCOM_64_3.0.1.5

*Release Date
Jan 04, 2013

*Software Type
 USB Virtual COM Driver

*Description
 Cino USB virtual COM driver supports FuzzyScan scan engines/scanners. It will create a virtual COM port in 
 the host, enabling the scanner work as a legacy RS232 serial device.   
 
*Supported Devices
 Scan Engines                       SE380, SE390
 Fixed Mount Scanners               FM480
 Corded Scanners                    F560, F680, F780, F790, L680, L780
 Bluetooth Scanners                 F680BT, F780BT, F790BT,L680BT, L780BT
 Wi-Fi Scanners                     F790WD, L780WD
 Area-Imaging ScannerS              A770 

*Supported Operating Systems: 
 Windows XP SP3 32/64 bit, Windows Vista SP2 32/64 bit and Windows 7 SP1 32/64 bit

